1. **INTRODUCTION**

Road safety is a paramount concern in today’s fast-paced world, where vehicular traffic continues to grow exponentially. One of the leading causes of traffic-related fatalities and accidents is driving under the influence of alcohol. According to the World Health Organization (WHO), approximately 1.3 million people die each year as a result of road traffic crashes, and alcohol consumption contributes significantly to this statistic. Despite widespread awareness campaigns, strict laws, and penalties, incidents of drunk driving remain alarmingly frequent. This calls for an effective, technological intervention to eliminate human negligence and reduce road mishaps. In addition to the legal and ethical implications, drunk driving also imposes a substantial economic burden on public health systems, insurance industries, and families affected by such tragedies.

The Alcohol Detection and Vehicle Control System Using Arduino has been conceptualized and developed as a preventive mechanism aimed at curbing such occurrences. The system is designed to restrict vehicle operation by actively monitoring the driver’s breath for alcohol content before allowing the engine to start. The project utilizes embedded technology, with Arduino Uno as the heart of the system, integrating it with an alcohol sensor, buzzer, relay module, motor, and LCD screen to simulate and control the vehicle’s ignition process. This cost-effective approach provides a compact and efficient way to implement real-time driver monitoring within personal or commercial vehicles, ensuring that intoxicated drivers are automatically deterred from operating a vehicle.

Traditionally, breathalyzer tests are conducted by law enforcement agencies after the vehicle is already in motion. These tests rely on human intervention, are not immediate, and have limited coverage. In contrast, this proposed system automatically screens the driver before the vehicle starts and immediately inhibits the ignition process if the alcohol concentration exceeds a safe threshold. This makes it a real-time, proactive solution that could significantly reduce accidents due to impaired driving. Furthermore, this system eliminates the need for external enforcement and operates autonomously, making it ideal for everyday use without disrupting the normal functioning of the vehicle.

The use of the MQ-3 sensor enables detection of ethanol vapor in the driver’s breath. The analog signal generated by the sensor is processed by the Arduino microcontroller to determine whether the detected alcohol level surpasses the programmed threshold. If it does, the relay module cuts off the power to the motor (representing the vehicle engine), the buzzer sounds an alert, and the LCD displays a warning message. This closed-loop system ensures that the vehicle remains immobile until the driver is sober. The system also logs these events using the serial monitor, enabling easy debugging and monitoring during testing and deployment.

The design also emphasizes modularity and power efficiency. The entire circuit is powered by a rechargeable 18650 lithium-ion battery, allowing the system to function even in portable or off-grid scenarios. The components are carefully selected to ensure low power consumption, ease of integration, and high reliability. Moreover, the system's I2C-based LCD interface minimizes pin usage, leaving room for future feature additions without hardware redesign. This efficient design philosophy enables the project to be scaled or adapted without extensive hardware or software overhaul.

As the project is built on an open-source platform, it can be further developed and customized. For instance, the system can be extended to include cloud connectivity via IoT platforms, GSM modules for sending emergency alerts to family or authorities, and GPS modules for vehicle tracking. It also lays the foundation for integration into commercial vehicle fleets and public transportation systems to enforce alcohol-free driving policies. Educational institutions and driving schools can use similar models to train and educate future drivers about responsible driving behavior and the implications of alcohol consumption.

In summary, this project serves not only as a functional prototype but also as a vision for safer roads through technological intervention. It showcases how microcontroller-based systems, when combined with appropriate sensors and control mechanisms, can address real-life challenges effectively. The Alcohol Detection and Vehicle Control System stands as a testament to the potential of embedded systems in making human lives safer and smarter. By focusing on prevention, rather than punishment, the system represents a shift toward compassionate, intelligent safety enforcement that encourages responsible behavior while ensuring public safety.

**2.LITERATURE SURVEY / RELATED WORK**

The issue of drunk driving has been a critical concern for governments, safety organizations, and automotive engineers worldwide. Numerous research projects and commercial implementations have attempted to address this challenge using different technological approaches. The literature survey for this project focuses on existing systems, their strengths and weaknesses, and how our proposed system offers improvements.

One of the most widely implemented systems in countries like the United States, Sweden, and Canada is the breathalyzer-based ignition interlock device. These systems are primarily installed in the vehicles of individuals with previous DUI offenses. Before starting the engine, the driver is required to blow into a breathalyzer device. If alcohol is detected above a preset threshold, the engine remains locked. Sweden's AlcoLock system, for instance, has shown significant success in reducing repeat DUI incidents by over 70%. However, these systems are expensive, intrusive, and are typically mandated only after a conviction rather than being proactively installed in all vehicles.

In India and other developing countries, preventive technology for drunk driving is still in its nascent stage. Most enforcement is carried out manually by traffic police through random breath tests. These checks, although effective to some extent, suffer from scalability issues, human error, and limited coverage. During peak hours or in remote areas, law enforcement presence is minimal, which reduces the effectiveness of such interventions.

Research initiatives have also been conducted in academic and industrial domains. Various studies have explored sensor-based systems that use gas sensors like MQ-3, MQ-135, and others to detect alcohol presence in the surrounding air. These sensors offer affordability and decent accuracy but are sensitive to environmental variables such as temperature, humidity, and cross-sensitivity to other gases. Improvements in calibration and enclosure design have helped mitigate some of these challenges.

Artificial intelligence and machine learning-based driver monitoring systems are another area of active research. These systems use cameras and AI algorithms to detect drowsiness, erratic behavior, and signs of intoxication based on facial recognition, head tilt, and eye movement. Companies like Toyota and Mercedes-Benz have integrated such systems into their high-end models. However, these solutions are costly and not easily deployable in budget-friendly vehicles or retrofittable to existing models.

More recently, research supported by the Driver Alcohol Detection System for Safety (DADSS) program in the USA aims to develop passive alcohol detection systems that require no active input from the driver. These systems use infrared sensors in the vehicle cabin to detect alcohol levels through ambient breath or skin contact. The goal is to create seamless systems that do not inconvenience the driver but still ensure safety. However, these systems are still under development and are not yet commercially available.

In comparison, the system proposed in this project strikes a balance between functionality, affordability, and ease of implementation. By using an Arduino Uno, MQ-3 sensor, a relay for control, and an LCD for user feedback, the system achieves all core functionalities of high-end interlock systems but at a fraction of the cost. It also addresses the challenge of manual enforcement by offering an autonomous, embedded, and scalable solution that can be deployed in both personal and commercial vehicles.

The proposed system is also open to integration with future technologies such as GSM for remote alerting, GPS for location tracking, and cloud-based data management. These possibilities make it a robust and adaptable system in the evolving landscape of automotive safety technologies.

In conclusion, while many systems exist for detecting alcohol and preventing drunk driving, there is a clear gap in affordable, standalone, and proactive safety mechanisms for the average driver. This project addresses that gap by building upon established methods and tailoring them for practical, widespread deployment in diverse vehicular environments.

**3. SYSTEM ANALASIS**

### 3.1 EXISTING SYSTEM

The existing systems for preventing drunk driving primarily fall into two broad categories: manual enforcement mechanisms and commercial breathalyzer interlock devices. Each of these systems has its own set of benefits and limitations, yet they still fall short in providing a universally applicable, low-cost, and proactive solution.

#### \* Manual Enforcement

In many countries, especially in developing regions, the predominant strategy for controlling drunk driving involves law enforcement personnel conducting random breathalyzer tests at checkpoints. Officers stop vehicles randomly and use handheld devices to test drivers for alcohol consumption. While effective in specific scenarios, this method suffers from several limitations:

**Limited Reach and Timing:** Officers cannot cover all areas or operate round-the-clock, making it impossible to detect all offenders.

**Human Dependency:** The effectiveness of manual enforcement is highly dependent on the diligence, training, and availability of traffic police.

**Inconvenience and Delay:** Random checks often cause traffic congestion and delay, leading to resistance and evasion from the public.

**Corruption Risk:** In regions where bribery is common, offenders may escape penalties, making the system unreliable.

#### \* Breathalyzer-Based Interlock Systems

In developed countries, repeat DUI offenders are often mandated to install alcohol detection ignition interlocks in their vehicles. These systems require the driver to blow into a breathalyzer before the vehicle can be started. If the alcohol content exceeds the legal limit, the system locks the ignition.While these systems offer automation and are proven to reduce repeat offenses, they also have significant downsides:

**High Cost:** These systems are expensive to install and maintain, limiting their accessibility to a wider population.

**Inconvenient for First-Time Users:** These are often perceived as punitive and are not typically installed proactively in personal or family vehicles.

**Limited Availability:** Mostly deployed in cases mandated by court orders, making them reactive rather than preventive.

#### \* Other Limitations of Existing Systems:

**Lack of Real-Time Detection:** Many systems only check alcohol levels once, during vehicle startup. There is no monitoring after the vehicle is in motion.

**Absence of Multi-Modal Alerts:** Most systems do not include audio-visual alerts or automated communication to guardians or emergency services.

**Complexity in Integration:** Advanced AI and sensor-based systems, although effective, require complex installation and are not compatible with all types of vehicles.

#### Summary

While existing systems have made progress in addressing drunk driving, they fall short of offering a real-time, low-cost, and user-friendly solution that can be widely adopted across various vehicle types and income groups. The existing setups either depend heavily on manual enforcement or are reserved for high-end applications. There remains a pressing need for a solution that is autonomous, easy to install, affordable, and capable of preventing intoxicated drivers from operating a vehicle before any harm can occur.

The proposed system addresses these issues by integrating readily available components into an embedded system that is both scalable and cost-effective, offering a much-needed bridge between low-tech manual systems and expensive high-tech commercial alternatives.

### 3.2 DISADVANTAGES OF EXISTING SYSTEM

* **Dependence on Manual Processes:** Most systems require human presence and intervention, which is inconsistent and limited in coverage.
* **Costly Installations:** Breathalyzer-based interlocks and AI-based systems are often expensive and not affordable for average consumers.
* **Non-Real-Time Monitoring:** Traditional systems do not provide continuous monitoring after vehicle ignition, allowing the possibility of drivers consuming alcohol after starting the vehicle.
* **Limited Enforcement Reach:** Police checkpoints can only cover a small percentage of drivers, leaving a large population unchecked.
* **Lack of User Feedback:** Existing systems rarely incorporate intuitive user interfaces or alerts that inform and guide the driver.
* **Poor Accessibility:** These systems are either confined to premium cars or mandated post-incident, with no universal or preventive implementation.

### 3.3 PROPOSED SYSTEM

The proposed system is an embedded, microcontroller-based Alcohol Detection and Vehicle Control mechanism designed to detect alcohol levels in a driver’s breath and automatically restrict the vehicle from starting if the levels exceed a predefined safety threshold. The system uses an MQ-3 alcohol sensor to detect ethanol vapors, an Arduino Uno microcontroller for data processing and control logic, a relay to simulate engine cut-off, and visual and audio feedback components such as an LCD and buzzer.

What sets this system apart is its dual-phase detection: it checks for alcohol both before the vehicle starts and during the vehicle's operation. This enables real-time prevention of accidents, even if a driver begins consuming alcohol after starting the vehicle. During startup, if alcohol is detected, the LCD will display a warning, the buzzer will sound an alarm, and the relay will cut off power to the motor. While driving, periodic checks continue in the background, and if alcohol is detected again, the vehicle is brought to a safe halt by gradually slowing down the motor.

In terms of usability, the system is compact, easy to integrate with minimal wiring, and has low power requirements, making it suitable for a wide range of vehicle types, from bikes to cars. Future enhancements such as GSM modules (to alert a guardian or emergency contact), GPS modules (for real-time location tracking), and IoT cloud integration (for data logging and analysis) can be easily added due to the open and expandable design.

This solution bridges the gap between expensive commercial interlock systems and manual enforcement, offering a practical, affordable, and real-world-ready preventive mechanism that promotes road safety at the grassroots level.

### 3.4 ADVANTAGES OF PROPOSED SYSTEM

* **Cost-Effective Solution:** Utilizes easily available, inexpensive components to create a highly functional and responsive alcohol detection system.
* **Autonomous Functionality:** Functions independently without the need for law enforcement or human supervision.
* **Real-Time Monitoring:** Continuously checks alcohol levels during vehicle operation to prevent mid-journey drinking and ensures safety throughout the drive.
* **Easy to Install:** Requires basic connections and minimal coding, allowing easy installation in both new and existing vehicles.
* **Audio-Visual Feedback:** Provides real-time alerts to the driver using a buzzer and LCD, making the interface user-friendly and informative.
* **Scalable Design:** Modular design allows for easy upgrades to include features like cloud connectivity, SMS alerts, or location tracking.
* **Eco-Friendly and Life-Saving:** Helps reduce road accidents and casualties due to drunk driving, ultimately promoting a safer and greener driving culture.

### 3.5 LIMITATIONS OF ADVANCED SYSTEM

While the proposed system offers several advantages, there are still some inherent limitations that must be acknowledged:

* **Sensor Sensitivity:** The MQ-3 sensor is susceptible to interference from other volatile compounds like perfumes, sanitizers, or smoke, leading to false positives.
* **Power Dependency:** As with all electronic systems, a continuous and stable power source is necessary. Battery depletion or faulty connections could disable the system.
* **Intrusiveness for Some Users:** Regular alcohol checks, even for non-intoxicated users, may be perceived as time-consuming or annoying, potentially discouraging use.
* **Environmental Constraints:** Extreme weather conditions such as excessive humidity or cold can affect sensor calibration and performance.
* **Tampering Risks:** Since the setup is exposed and relatively simple, users could attempt to bypass the sensor using external air or obstructions, although this can be addressed with better casing and placement.

Despite these challenges, the proposed system marks a significant leap forward in proactive driver safety systems, particularly for budget-conscious consumers and emerging markets. The flexibility of the design ensures that many of these limitations can be overcome with future enhancements or version upgrades.

**4.SYSTEM STUDY**

The development of the Alcohol Detection and Vehicle Control System requires a comprehensive understanding of the operational environment, the end-user requirements, the technical feasibility, and the socio-economic implications. A thorough system study serves as the backbone of the design and development phase, ensuring the proposed system effectively addresses the shortcomings of existing solutions and fulfills the intended purpose.

Drunk driving is a global issue responsible for thousands of preventable deaths every year. Conventional approaches like law enforcement and breathalyzer tests, while useful, do not provide a continuous or automated solution. This gap highlights the necessity for an integrated, technology-driven system that can detect alcohol consumption in real time and act immediately to prevent the driver from operating a vehicle. The Alcohol Detection and Vehicle Control System attempts to fill this gap by leveraging embedded systems and automation.

The system study aims to investigate all the components involved in this solution, from conceptualization to implementation. It evaluates the logical and physical structure of the system, user interaction, and the response behavior based on input from real-world scenarios. The ultimate goal is to ensure that the solution is practical, efficient, cost-effective, and scalable for different types of vehicles.

This project proposes using an Arduino Uno microcontroller as the core component, interfaced with an MQ-3 alcohol sensor that can detect ethanol vapor in the breath. When the alcohol level exceeds a defined safety threshold, the system will immediately trigger a buzzer, display a warning on an LCD screen, and deactivate the relay module that simulates cutting off the car's ignition. These functionalities are designed to stop a driver from starting or continuing to drive under the influence.

The system study involves the following critical aspects:

* **Identification of real-world challenges:** Recognizing the high rate of alcohol-related accidents and the inability of existing systems to offer preventive, real-time action at the grassroots level.
* **Understanding user requirements:** Aiming for a non-intrusive, user-friendly solution that works automatically and does not inconvenience sober drivers.
* **Component selection and integration:** Selecting components like the MQ-3 sensor for reliable alcohol detection, Arduino Uno for logic processing, LCD for display, buzzer for audible alerts, and relay for controlling power to the motor (representing vehicle ignition). This selection ensures cost-effectiveness, accuracy, and simplicity.
* **Feasibility and reliability:** Studying hardware durability, environmental adaptability, power efficiency, and real-world usability to ensure consistent system performance.
* **Flexibility for expansion:** Considering future upgrades such as GSM modules to send SMS alerts to guardians or emergency services, GPS for location tracking, and cloud connectivity for remote data monitoring.

In terms of implementation, the system is structured in two phases:

* **Pre-Ignition Phase:** The driver is prompted to blow air near the sensor before the car is started. If alcohol is detected, the motor does not run, and warning signals are activated.
* **Post-Ignition Monitoring:** If the car is already running, the system continues monitoring at intervals. If intoxication is detected mid-journey, the system gradually halts the vehicle and triggers warnings.

This intelligent behavior ensures the system not only blocks the initial operation of the vehicle by a drunk driver but also prevents situations where a driver consumes alcohol after starting the vehicle.

From a socio-economic perspective, the system has the potential to significantly reduce the risk of accidents, save lives, and reduce public expenditure on emergency services, insurance claims, and legal proceedings. Furthermore, the project promotes responsible driving behavior and opens up avenues for its adoption in school transportation, logistics fleets, and personal vehicles.

In conclusion, the system study provides a comprehensive view of the proposed solution, focusing on its relevance, feasibility, and potential impact. It lays a solid foundation for the design, development, testing, and deployment of a robust and scalable alcohol detection system for vehicles. This project envisions not only an enhancement in technical capability but also a meaningful contribution to public health and safety through preventive technology.

**5.HARDWARE AND SOFTWARE REQUIREMENTS**

To develop and implement the Alcohol Detection and Vehicle Control System effectively, both hardware and software resources are crucial. These components form the core infrastructure of the project, enabling real-time sensing, decision-making, alert generation, and system response.

### 5.1 HARDWARE REQUIREMENTS


The following are the essential hardware components required for the prototype:

**\* Arduino Uno:**

The **Arduino Uno** is a series of [open-source](https://en.wikipedia.org/wiki/Open-source" \o "Open-source) [microcontroller board](https://en.wikipedia.org/wiki/Single-board_microcontroller" \o "Single-board microcontroller) based on a diverse range of [microcontrollers](https://en.wikipedia.org/wiki/Microcontroller" \o "Microcontroller) (MCU). It was initially developed and released by [Arduino](https://en.wikipedia.org/wiki/Arduino" \o "Arduino) company in 2010. The [microcontroller board](https://en.wikipedia.org/wiki/Single-board_microcontroller" \o "Single-board microcontroller) is equipped with sets of digital and analog [input/output](https://en.wikipedia.org/wiki/Input/output" \o "Input/output) (I/O) pins that may be interfaced to various [expansion boards](https://en.wikipedia.org/wiki/Expansion_board" \o "Expansion board) (shields) and other circuits.The board has 14 digital I/O pins (six capable of [PWM](https://en.wikipedia.org/wiki/Pulse-width_modulation" \o "Pulse-width modulation) output), 6 analog I/O pins, and is programmable with the [Arduino IDE](https://en.wikipedia.org/wiki/Arduino" \l "Software" \o "Arduino) (Integrated Development Environment), via a type B [USB cable](https://en.wikipedia.org/wiki/USB_cable" \o "USB cable).It can be powered by a USB cable or a barrel connector that accepts voltages between 7 and 20 volts, such as a rectangular [9-volt battery](https://en.wikipedia.org/wiki/9-volt_battery" \o "9-volt battery). It has the same microcontroller as the [Arduino Nano](https://en.wikipedia.org/wiki/Arduino_Nano" \o "Arduino Nano) board, and the same headers as the Leonardo board. The hardware reference design is distributed under a [Creative Commons](https://en.wikipedia.org/wiki/Creative_Commons" \o "Creative Commons) Attribution Share-Alike 2.5 license and is available on the Arduino website. Layout and production files for some versions of the hardware are also available.

The word "[uno](https://en.wiktionary.org/wiki/uno" \o "wikt:uno)" means "one" in [Italian](https://en.wikipedia.org/wiki/Italian_language" \o "Italian language) and was chosen to mark a major redesign of the Arduino hardware and software. The Uno board was the successor of the Duemilanove release and was the 9th version in a series of USB-based Arduino boards. Version 1.0 of the Arduino [IDE](https://en.wikipedia.org/wiki/Integrated_development_environment" \o "Integrated development environment) for the Arduino Uno board has now evolved to newer releases. The ATmega328 on the board comes preprogrammed with a [bootloader](https://en.wikipedia.org/wiki/Bootloader" \o "Bootloader) that allows uploading new code to it without the use of an external hardware programmer.

While the Uno communicates using the original STK500 protocol, it differs from all preceding boards in that it does not use a [FTDI](https://en.wikipedia.org/wiki/FTDI" \o "FTDI) USB-to-UART serial chip. Instead, it uses the Atmega16U2 (Atmega8U2 up to version R2) programmed as a [USB-to-serial converter](https://en.wikipedia.org/wiki/USB-to-serial_converter" \o "USB-to-serial converter).

**A.Arduino Uno**

**\* MQ-3 Alcohol Sensor:**

The MQ3 gas sensor is alcohol sensor which is used to detect the alcohol concentration on your breath.This sensor provides an analog resistive output based on alcohol concentration. When the alcohol gas exist, the sensor’s conductivity gets higher along with the gas concentration rising.It is suitable for various applications of detecting alcohol at different concentration.It is widely used in domestic alcohol gas alarm, industrial alcohol gas alarm and portable alcohol detector. Specifications: Supply Voltage: 5V Detecting Concentration:0.05-10mg/L Alcohol Analog and Digital Output Digital Out is High or Low based on a adjustable preset threshold.

B.**MQ-3 Alcohol Sensor**

**\* Relay Module (5V):**

A **relay** is an [electrically](https://en.wikipedia.org/wiki/Electric" \o "Electric) operated [switch](https://en.wikipedia.org/wiki/Switch" \o "Switch). It consists of a set of input terminals for a single or multiple [control signals](https://en.wikipedia.org/wiki/Signaling_(telecommunications)" \o "Signaling (telecommunications)), and a set of operating contact terminals. The switch may have any number of contacts in multiple [contact forms](https://en.wikipedia.org/wiki/Electrical_contact" \l "Contact_form" \o "Electrical contact), such as make contacts, break contacts, or combinations thereof.

Relays are used where it is necessary to control a circuit by an independent low-power signal, or where several circuits must be controlled by one signal. Relays were first used in long-distance [telegraph](https://en.wikipedia.org/wiki/Electrical_telegraph" \o "Electrical telegraph) circuits as signal repeaters: they refresh the signal coming in from one circuit by transmitting it on another circuit. Relays were used extensively in [telephone exchanges](https://en.wikipedia.org/wiki/Telephone_exchange" \o "Telephone exchange) and early [computers](https://en.wikipedia.org/wiki/Computer" \o "Computer) to perform logical operations.

The traditional [electromechanical](https://en.wikipedia.org/wiki/Electromechanical" \o "Electromechanical) form of a relay uses an [electromagnet](https://en.wikipedia.org/wiki/Electromagnet" \o "Electromagnet) to close or open the contacts, but relays using other operating principles have also been invented, such as in [solid-state relays](https://en.wikipedia.org/wiki/Solid-state_relay" \o "Solid-state relay) which use [semiconductor](https://en.wikipedia.org/wiki/Semiconductor" \o "Semiconductor) properties for control without relying on [moving parts](https://en.wikipedia.org/wiki/Moving_parts" \o "Moving parts). Relays with calibrated operating characteristics and sometimes multiple operating coils are used to protect [electrical circuits](https://en.wikipedia.org/wiki/Electrical_network" \o "Electrical network) from overload or faults; in modern electric power systems these functions are performed by digital instruments still called *[protective relays](https://en.wikipedia.org/wiki/Protective_relay" \o "Protective relay)* or *[safety relays](https://en.wikipedia.org/wiki/Safety_relay" \o "Safety relay)*.

Latching relays require only a single pulse of control power to operate the switch persistently. Another pulse applied to a second set of control terminals, or a pulse with opposite polarity, resets the switch, while repeated pulses of the same kind have no effects. Magnetic latching relays are useful in applications when interrupted power should not affect the circuits that the relay is controlling.

C.**Relay Module (5V)**

**\* DC Motor or Model Engine:**

A **DC motor** is an [electrical motor](https://en.wikipedia.org/wiki/Electrical_motor" \o "Electrical motor) that uses direct current (DC) to produce mechanical force. The most common types rely on magnetic forces produced by currents in the coils. Nearly all types of DC motors have some internal mechanism, either electromechanical or electronic, to periodically change the direction of current in part of the motor.

DC motors were the first form of motors to be widely used, as they could be powered from existing direct-current lighting power distribution systems. A DC motor's speed can be controlled over a wide range, using either a variable supply voltage or by changing the strength of current in its field windings. Small DC motors are used in tools, toys, and appliances. The [universal motor](https://en.wikipedia.org/wiki/Universal_motor" \o "Universal motor), a lightweight [brushed](https://en.wikipedia.org/wiki/Brush_(electric)" \o "Brush (electric)) motor used for portable power tools and appliances can operate on direct current and alternating current. Larger DC motors are currently used in propulsion of electric vehicles, elevator and hoists, and in drives for steel rolling mills. The advent of [power electronics](https://en.wikipedia.org/wiki/Power_electronics" \o "Power electronics) has made replacement of DC motors with [AC motors](https://en.wikipedia.org/wiki/AC_motors" \o "AC motors) possible in many applications.

D.**DC Motor**

**\* LCD Display (16x2 or I2C):**

A **liquid-crystal display** (**LCD**) is a [flat-panel display](https://en.wikipedia.org/wiki/Flat-panel_display" \o "Flat-panel display) or other [electronically modulated optical device](https://en.wikipedia.org/wiki/Electro-optic_modulator" \o "Electro-optic modulator) that uses the light-modulating properties of [liquid crystals](https://en.wikipedia.org/wiki/Liquid_crystal" \o "Liquid crystal) combined with [polarizers](https://en.wikipedia.org/wiki/Polarizer" \o "Polarizer) to display information. Liquid crystals do not emit light directly[[1]](https://en.wikipedia.org/wiki/Liquid-crystal_display" \l "cite_note-1) but instead use a [backlight](https://en.wikipedia.org/wiki/Backlight" \o "Backlight) or [reflector](https://en.wikipedia.org/wiki/Reflector_(photography)" \o "Reflector (photography)) to produce images in color or [monochrome](https://en.wikipedia.org/wiki/Monochrome_monitor" \o "Monochrome monitor).[[2]](https://en.wikipedia.org/wiki/Liquid-crystal_display" \l "cite_note-2)

LCDs are available to display arbitrary images (as in a general-purpose computer display) or fixed images with low information content, which can be displayed or hidden: preset words, digits, and [seven-segment displays](https://en.wikipedia.org/wiki/Seven-segment_display" \o "Seven-segment display) (as in a digital clock) are all examples of devices with these displays. They use the same basic technology, except that arbitrary images are made from a matrix of small [pixels](https://en.wikipedia.org/wiki/Pixel" \o "Pixel), while other displays have larger elements.

LCDs are used in a wide range of applications, including [LCD televisions](https://en.wikipedia.org/wiki/LCD_television" \o "LCD television), [computer monitors](https://en.wikipedia.org/wiki/Computer_monitor" \o "Computer monitor), [instrument panels](https://en.wikipedia.org/wiki/Dashboard" \o "Dashboard), [aircraft cockpit displays](https://en.wikipedia.org/wiki/Flight_instruments" \o "Flight instruments), and indoor and outdoor signage. Small LCD screens are common in [LCD projectors](https://en.wikipedia.org/wiki/LCD_projector" \o "LCD projector) and portable consumer devices such as [digital cameras](https://en.wikipedia.org/wiki/Digital_camera" \o "Digital camera), [watches](https://en.wikipedia.org/wiki/Watch" \o "Watch), [calculators](https://en.wikipedia.org/wiki/Calculator" \o "Calculator), and [mobile telephones](https://en.wikipedia.org/wiki/Mobile_phone" \o "Mobile phone), including [smartphones](https://en.wikipedia.org/wiki/Smartphone" \o "Smartphone). LCD screens have replaced heavy, bulky and less energy-efficient [cathode-ray tube](https://en.wikipedia.org/wiki/Cathode-ray_tube" \o "Cathode-ray tube) (CRT) displays in nearly all applications since the late 2000s to the early 2010s.

LCDs can either be normally on (positive) or off (negative), depending on the polarizer arrangement. For example, a character positive LCD with a backlight has black lettering on a background that is the color of the backlight, and a character negative LCD has a black background with the letters being of the same color as the backlight.

LCDs are not subject to [screen burn-in](https://en.wikipedia.org/wiki/Screen_burn-in" \o "Screen burn-in) like on CRTs. However, LCDs are still susceptible to [image persistence](https://en.wikipedia.org/wiki/Image_persistence" \o "Image persistence).[[3]](https://en.wikipedia.org/wiki/Liquid-crystal_display" \l "cite_note-Fujitsu-3)



E. **LCD Display (16x2 or I2C)**

**\* Buzzer:**

A **buzzer** or **beeper** is an [audio](https://en.wikipedia.org/wiki/Sound" \o "Sound) signaling device,[[1]](https://en.wikipedia.org/wiki/Buzzer" \l "cite_note-1) which may be [mechanical](https://en.wikipedia.org/wiki/Machine" \o "Machine), [electromechanical](https://en.wikipedia.org/wiki/Electromechanics" \o "Electromechanics), or [piezoelectric](https://en.wikipedia.org/wiki/Piezoelectricity" \o "Piezoelectricity) (*piezo* for short). Typical uses of buzzers and beepers include [alarm devices](https://en.wikipedia.org/wiki/Alarm_devices" \o "Alarm devices), [timers](https://en.wikipedia.org/wiki/Timer" \o "Timer), [train](https://en.wikipedia.org/wiki/Train" \o "Train) and confirmation of user input such as a mouse click or keystroke.

F.**Buzzer**

**\* LED (Optional):**

A **light-emitting diode** (**LED**) is a [semiconductor device](https://en.wikipedia.org/wiki/Semiconductor_device" \o "Semiconductor device) that [emits light](https://en.wikipedia.org/wiki/Light" \l "Light_sources" \o "Light) when [current](https://en.wikipedia.org/wiki/Electric_current" \o "Electric current) flows through it. [Electrons](https://en.wikipedia.org/wiki/Electron" \o "Electron) in the semiconductor recombine with [electron holes](https://en.wikipedia.org/wiki/Electron_hole" \o "Electron hole), releasing energy in the form of [photons](https://en.wikipedia.org/wiki/Photon" \o "Photon). The color of the light (corresponding to the energy of the photons) is determined by the energy required for electrons to cross the [band gap](https://en.wikipedia.org/wiki/Band_gap" \o "Band gap) of the [semiconductor](https://en.wikipedia.org/wiki/Semiconductor" \o "Semiconductor).[[5]](https://en.wikipedia.org/wiki/Light-emitting_diode" \l "cite_note-5) White light is obtained by using multiple semiconductors or a layer of light-emitting [phosphor](https://en.wikipedia.org/wiki/Phosphor" \o "Phosphor) on the semiconductor device.[[6]](https://en.wikipedia.org/wiki/Light-emitting_diode" \l "cite_note-6)

Appearing as practical electronic components in 1962, the earliest LEDs emitted low-intensity [infrared](https://en.wikipedia.org/wiki/Infrared" \o "Infrared) (IR) light.[[7]](https://en.wikipedia.org/wiki/Light-emitting_diode" \l "cite_note-FirstPracticalLED-7) Infrared LEDs are used in [remote-control](https://en.wikipedia.org/wiki/Remote_control" \o "Remote control) circuits, such as those used with a wide variety of consumer electronics. The first visible-light LEDs were of low intensity and limited to red.

Early LEDs were often used as indicator lamps, replacing small [incandescent bulbs](https://en.wikipedia.org/wiki/Incandescent_light_bulb" \o "Incandescent light bulb), and in [seven-segment displays](https://en.wikipedia.org/wiki/Seven-segment_display" \o "Seven-segment display). Later developments produced LEDs available in [visible](https://en.wikipedia.org/wiki/Visible_spectrum" \o "Visible spectrum), [ultraviolet](https://en.wikipedia.org/wiki/Ultraviolet" \o "Ultraviolet) (UV), and infrared wavelengths with high, low, or intermediate light output, for instance, white LEDs suitable for room and outdoor lighting. LEDs have also given rise to new types of displays and sensors, while their high switching rates are useful in advanced communications technology. LEDs have been used in diverse applications such as [aviation lighting](https://en.wikipedia.org/wiki/Navigation_light" \o "Navigation light), [fairy lights](https://en.wikipedia.org/wiki/Christmas_lights" \o "Christmas lights), [strip lights](https://en.wikipedia.org/wiki/LED_strip_light" \o "LED strip light), [automotive headlamps](https://en.wikipedia.org/wiki/Automotive_lighting" \l "Light-emitting_diodes_(LED)" \o "Automotive lighting), advertising, [stage lighting](https://en.wikipedia.org/wiki/Stage_lighting" \o "Stage lighting), [general lighting](https://en.wikipedia.org/wiki/Lighting" \o "Lighting), [traffic signals](https://en.wikipedia.org/wiki/Traffic_light" \o "Traffic light), camera flashes, [lighted wallpaper](https://en.wikipedia.org/wiki/LED_wallpaper" \o "LED wallpaper), [horticultural grow lights](https://en.wikipedia.org/wiki/Grow_light" \o "Grow light), and medical devices.[[8]](https://en.wikipedia.org/wiki/Light-emitting_diode" \l "cite_note-Aguilar-8)

LEDs have many advantages over incandescent light sources, including lower power consumption, a longer lifetime, improved physical robustness, smaller sizes, and faster switching. In exchange for these generally favorable attributes, disadvantages of LEDs include electrical limitations to low voltage and generally to DC (not AC) power, the inability to provide steady illumination from a pulsing DC or an AC electrical supply source, and a lesser maximum operating temperature and storage temperature.

LEDs are [transducers](https://en.wikipedia.org/wiki/Transducer" \o "Transducer) of electricity into light. They operate in reverse of [photodiodes](https://en.wikipedia.org/wiki/Photodiode" \o "Photodiode), which convert light into electricity.

G.LED

**\* Power Supply (Battery/USB):**

A **power supply** is an electrical device that supplies [electric power](https://en.wikipedia.org/wiki/Electric_power" \o "Electric power) to an [electrical load](https://en.wikipedia.org/wiki/Electrical_load" \o "Electrical load). The main purpose of a power supply is to convert [electric current](https://en.wikipedia.org/wiki/Electric_current" \o "Electric current) from a source to the correct [voltage](https://en.wikipedia.org/wiki/Voltage" \o "Voltage), [current](https://en.wikipedia.org/wiki/Electric_current" \o "Electric current), and [frequency](https://en.wikipedia.org/wiki/Frequency" \o "Frequency) to power the load. As a result, power supplies are sometimes referred to as [electric power converters](https://en.wikipedia.org/wiki/Electric_power_converter" \o "Electric power converter). Some power supplies are separate standalone pieces of equipment, while others are built into the load appliances that they power. Examples of the latter include power supplies found in [desktop computers](https://en.wikipedia.org/wiki/Desktop_computer" \o "Desktop computer) and [consumer electronics](https://en.wikipedia.org/wiki/Consumer_electronics" \o "Consumer electronics) devices. Other functions that power supplies may perform include limiting the current drawn by the load to safe levels, shutting off the current in the event of an [electrical fault](https://en.wikipedia.org/wiki/Electrical_fault" \o "Electrical fault), power conditioning to prevent [electronic noise](https://en.wikipedia.org/wiki/Electronic_noise" \o "Electronic noise) or [voltage surges](https://en.wikipedia.org/wiki/Voltage_surge" \o "Voltage surge) on the input from reaching the load, [power-factor correction](https://en.wikipedia.org/wiki/Power-factor_correction" \o "Power-factor correction), and storing energy so it can continue to power the load in the event of a temporary interruption in the source power ([uninterruptible power supply](https://en.wikipedia.org/wiki/Uninterruptible_power_supply" \o "Uninterruptible power supply)).

****All power supplies have a *power input* connection, which receives energy in the form of electric current from a source, and one or more *power output* or **power rail** connections that deliver current to the load. The source power may come from the [electric power grid](https://en.wikipedia.org/wiki/Electric_power_grid" \o "Electric power grid), such as an [electrical outlet](https://en.wikipedia.org/wiki/Electrical_outlet" \o "Electrical outlet), [energy storage](https://en.wikipedia.org/wiki/Energy_storage" \o "Energy storage) devices such as [batteries](https://en.wikipedia.org/wiki/Battery_(electricity)" \o "Battery (electricity)) or [fuel cells](https://en.wikipedia.org/wiki/Fuel_cell" \o "Fuel cell), [generators](https://en.wikipedia.org/wiki/Electrical_generators" \o "Electrical generators) or [alternators](https://en.wikipedia.org/wiki/Alternator" \o "Alternator), [solar power](https://en.wikipedia.org/wiki/Solar_power" \o "Solar power) converters, or another power supply. The input and output are usually hardwired circuit connections, though some power supplies employ [wireless energy transfer](https://en.wikipedia.org/wiki/Wireless_power" \o "Wireless power) to power their loads without wired connections. Some power supplies have other types of inputs and outputs as well, for functions such as external monitoring and control.

H.**Power Supply**

**\*USB :**

**Universal Serial Bus** (**USB**) is an [industry standard](https://en.wikipedia.org/wiki/Technical_standard" \o "Technical standard), developed by [USB Implementers Forum](https://en.wikipedia.org/wiki/USB_Implementers_Forum" \o "USB Implementers Forum) (USB-IF), for digital data transmission and power delivery between many types of electronics. It specifies the architecture, in particular the physical [interfaces](https://en.wikipedia.org/wiki/Interface_(computing)" \o "Interface (computing)), and [communication protocols](https://en.wikipedia.org/wiki/Communication_protocol" \o "Communication protocol) to and from *hosts*, such as [personal computers](https://en.wikipedia.org/wiki/Personal_computer" \o "Personal computer), to and from [peripheral](https://en.wikipedia.org/wiki/Peripheral" \o "Peripheral) *devices*, e.g. displays, keyboards, and mass storage devices, and to and from intermediate *hubs*, which multiply the number of a host's ports.[[2]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB42Spec-2)

Introduced in 1996, USB was originally designed to standardize the connection of peripherals to computers, replacing various interfaces such as [serial ports](https://en.wikipedia.org/wiki/Serial_port" \o "Serial port), [parallel ports](https://en.wikipedia.org/wiki/Parallel_port" \o "Parallel port), [game ports](https://en.wikipedia.org/wiki/Game_port" \o "Game port), and [Apple Desktop Bus](https://en.wikipedia.org/wiki/Apple_Desktop_Bus" \o "Apple Desktop Bus) (ADB) ports.[[3]](https://en.wikipedia.org/wiki/USB" \l "cite_note-3) Early versions of USB became commonplace on a wide range of devices, such as keyboards, mice, cameras, printers, scanners, flash drives, smartphones, game consoles, and power banks.[[4]](https://en.wikipedia.org/wiki/USB" \l "cite_note-4) USB has since evolved into a standard to replace virtually all common ports on computers, mobile devices, peripherals, power supplies, and manifold other small electronics.

In the latest standard, the [USB-C](https://en.wikipedia.org/wiki/USB-C" \o "USB-C) connector replaces many types of connectors for power (up to 240 W), displays (e.g. DisplayPort, HDMI), and many other uses, as well as all previous USB connectors.

As of 2024, USB consists of four generations of specifications: [USB 1.](https://en.wikipedia.org/wiki/USB" \l "USB_1.x)*[x](https://en.wikipedia.org/wiki/USB" \l "USB_1.x)*, [USB 2.0](https://en.wikipedia.org/wiki/USB" \l "USB_2.0), [USB 3.](https://en.wikipedia.org/wiki/USB_3.0" \o "USB 3.0)*[x](https://en.wikipedia.org/wiki/USB_3.0" \o "USB 3.0)*, and [USB4](https://en.wikipedia.org/wiki/USB4" \o "USB4). The USB4 specification enhances the data transfer and power delivery functionality with "a connection-oriented tunneling architecture designed to combine multiple protocols onto a single physical interface so that the total speed and performance of the USB4 Fabric can be dynamically shared."[[2]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB42Spec-2) In particular, USB4 supports the tunneling of the [Thunderbolt 3](https://en.wikipedia.org/wiki/Thunderbolt_(interface)" \o "Thunderbolt (interface)) protocols, namely [PCI Express](https://en.wikipedia.org/wiki/PCI_Express" \o "PCI Express) (PCIe, load/store interface) and [DisplayPort](https://en.wikipedia.org/wiki/DisplayPort" \o "DisplayPort) (display interface). USB4 also adds host-to-host interfaces.[[2]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB42Spec-2)

Each specification sub-version supports different [signaling rates](https://en.wikipedia.org/wiki/Signaling_rate" \o "Signaling rate) from 1.5 and 12 Mbit/s [half-duplex](https://en.wikipedia.org/wiki/Duplex_(telecommunications)" \l "Half_duplex" \o "Duplex (telecommunications)) in USB 1.0/1.1 to 80 Gbit/s [full-duplex](https://en.wikipedia.org/wiki/Duplex_(telecommunications)" \l "Full_duplex" \o "Duplex (telecommunications)) in USB4 2.0.[[5]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB31Spec-5)[[6]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB2Spec-6)[[7]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB32101Spec-7)[[2]](https://en.wikipedia.org/wiki/USB" \l "cite_note-USB42Spec-2) USB also provides power to peripheral devices; the latest versions of the standard extend the power delivery limits for battery charging and devices requiring up to 240 watts as defined in [USB Power Delivery (USB-PD)](https://en.wikipedia.org/wiki/USB_hardware" \l "USB_Power_Delivery" \o "USB hardware) Rev. V3.1.[[8]](https://en.wikipedia.org/wiki/USB" \l "cite_note-PDSpec-8) Over the years, USB(-PD) has been adopted as the standard power supply and charging format for many mobile devices, such as mobile phones, reducing the need for proprietary chargers.[[9]](https://en.wikipedia.org/wiki/USB" \l "cite_note-9)




**I.USB**

**\* Breadboard :**

A **breadboard**, **solderless breadboard**, or **protoboard** is a construction base used to build semi-permanent [prototypes](https://en.wikipedia.org/wiki/Electronic_prototype" \o "Electronic prototype) of [electronic circuits](https://en.wikipedia.org/wiki/Electronic_circuit" \o "Electronic circuit). Unlike a [perfboard](https://en.wikipedia.org/wiki/Perfboard" \o "Perfboard) or [stripboard](https://en.wikipedia.org/wiki/Stripboard" \o "Stripboard), breadboards do not require [soldering](https://en.wikipedia.org/wiki/Soldering" \o "Soldering) or destruction of tracks and are hence reusable. For this reason, breadboards are also popular with students and in technological education.

A variety of electronic systems may be prototyped by using breadboards, from small analog and digital circuits to complete [central processing units](https://en.wikipedia.org/wiki/Central_processing_unit" \o "Central processing unit) (CPUs).

Compared to more permanent circuit connection methods, modern breadboards have high [parasitic capacitance](https://en.wikipedia.org/wiki/Parasitic_capacitance" \o "Parasitic capacitance), relatively high resistance, and less reliable connections, which are subject to jostle and physical degradation. Signaling is limited to about 10 MHz, and even well below that frequency not everything works properly.



J.Breadboard

**\* Jumping wires :**

A **jump wire** (also known as **jumper**, **jumper wire**, **DuPont wire**) is an [electrical wire](https://en.wikipedia.org/wiki/Electrical_wire" \o "Electrical wire), or group of them in a cable, with a connector or pin at each end (or sometimes without them – simply "tinned"), which is normally used to interconnect the components of a [breadboard](https://en.wikipedia.org/wiki/Breadboard" \o "Breadboard) or other prototype or test circuit, internally or with other equipment or components, without soldering.[[1]](https://en.wikipedia.org/wiki/Jump_wire" \l "cite_note-1)

Individual jump wires are fitted by inserting their "end connectors" into the slots provided in a breadboard, the [header connector](https://en.wikipedia.org/wiki/Pin_header" \o "Pin header) of a circuit board, or a piece of test equipment.




**k.Jumping wires**

**\* Resistors (e.g., 330 ohm, 1K):** A **resistor** is a [passive](https://en.wikipedia.org/wiki/Passivity_(engineering)" \o "Passivity (engineering)) [two-terminal](https://en.wikipedia.org/wiki/Terminal_(electronics)" \o "Terminal (electronics)) [electronic component](https://en.wikipedia.org/wiki/Electronic_component" \o "Electronic component) that implements [electrical resistance](https://en.wikipedia.org/wiki/Electrical_resistance" \o "Electrical resistance) as a circuit element. In electronic circuits, resistors are used to reduce current flow, adjust signal levels, to [divide voltages](https://en.wikipedia.org/wiki/Voltage_divider" \o "Voltage divider), [bias](https://en.wikipedia.org/wiki/Biasing" \o "Biasing) active elements, and terminate [transmission lines](https://en.wikipedia.org/wiki/Transmission_line" \o "Transmission line), among other uses. High-power resistors that can dissipate many [watts](https://en.wikipedia.org/wiki/Watt" \o "Watt) of electrical power as heat may be used as part of motor controls, in power distribution systems, or as test loads for [generators](https://en.wikipedia.org/wiki/Electric_generator" \o "Electric generator). Fixed resistors have resistances that only change slightly with temperature, time or operating voltage. Variable resistors can be used to adjust circuit elements (such as a volume control or a lamp dimmer), or as sensing devices for heat, light, humidity, force, or chemical activity.

Resistors are common elements of [electrical networks](https://en.wikipedia.org/wiki/Electrical_network" \o "Electrical network) and [electronic circuits](https://en.wikipedia.org/wiki/Electronic_circuit" \o "Electronic circuit) and are ubiquitous in [electronic equipment](https://en.wikipedia.org/wiki/Electronics" \o "Electronics). Practical resistors as discrete components can be composed of various compounds and forms. Resistors are also implemented within [integrated circuits](https://en.wikipedia.org/wiki/Integrated_circuit" \o "Integrated circuit).

The electrical function of a resistor is specified by its resistance: common commercial resistors are manufactured over a range of more than nine [orders of magnitude](https://en.wikipedia.org/wiki/Orders_of_magnitude" \o "Orders of magnitude). The nominal value of the resistance falls within the [manufacturing tolerance](https://en.wikipedia.org/wiki/Engineering_tolerance" \l "Electrical_component_tolerance" \o "Engineering tolerance), indicated on the component.



### **L.Resistors**

**\*ESP 8266**:

The **ESP8266** is a low-cost [Wi-Fi](https://en.wikipedia.org/wiki/Wi-Fi" \o "Wi-Fi) microcontroller, with built-in [TCP/IP networking software](https://en.wikipedia.org/wiki/TCP/IP_stack" \o "TCP/IP stack), and [microcontroller](https://en.wikipedia.org/wiki/Microcontroller" \o "Microcontroller) capability, produced by [Espressif Systems](https://en.wikipedia.org/wiki/Espressif_Systems" \o "Espressif Systems)[[1]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-Espressif_ESP8266-1) in Shanghai, China.


The chip was popularized in the English-speaking [maker](https://en.wikipedia.org/wiki/Maker_culture" \o "Maker culture) community in August 2014 via the **ESP-01** module, made by a third-party manufacturer Ai-Thinker. This small module allows microcontrollers to connect to a Wi-Fi network and make simple TCP/IP connections using [Hayes](https://en.wikipedia.org/wiki/Hayes_command_set" \o "Hayes command set)-style commands. However, at first, there was almost no English-language documentation on the chip and the commands it accepted.[[2]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-2) The very low price and the fact that there were very few external components on the module, which suggested that it could eventually be very inexpensive in volume, attracted many hackers to explore the module, the chip, and the software on it, as well as to translate the Chinese documentation.[[3]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-3)

The **ESP8285** is a similar chip with a built-in 1 MiB flash memory, allowing the design of single-chip devices capable of connecting via Wi-Fi.[[4]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-esp8285-4)

These microcontroller chips have been succeeded by the [ESP32](https://en.wikipedia.org/wiki/ESP32" \o "ESP32) family of devices.

## Features


[[edit](https://en.wikipedia.org/w/index.php?title=ESP8266&action=edit&section=1" \o "Edit section: Features)]

[](https://en.wikipedia.org/wiki/File:ESP-01_Wireframe.png)

M.ESP-01 module wireframe drawing

* Processor: L106 32-bit [RISC](https://en.wikipedia.org/wiki/Reduced_instruction_set_computing" \o "Reduced instruction set computing) microprocessor core based on the [Tensilica](https://en.wikipedia.org/wiki/Tensilica" \o "Tensilica) Diamond Standard 106Micro running at 80 or 160 MHz[[5]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-5)
* Memory:[[6]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-memory-6)
  + 32 KiB instruction RAM
  + 32 KiB instruction cache RAM
  + 80 KiB user-data RAM
  + 16 KiB ETS system-data RAM
* External QSPI flash: up to 16 MiB is supported (512 KiB to 4 MiB typically included)
* [IEEE 802.11](https://en.wikipedia.org/wiki/IEEE_802.11" \o "IEEE 802.11) b/g/n [Wi-Fi](https://en.wikipedia.org/wiki/Wi-Fi" \o "Wi-Fi)
  + Integrated [TR switch](https://en.wikipedia.org/wiki/Duplexer" \l "Transmit-receive_switch" \o "Duplexer), [balun](https://en.wikipedia.org/wiki/Balun" \o "Balun), [LNA](https://en.wikipedia.org/wiki/Low-noise_amplifier" \o "Low-noise amplifier), [power amplifier](https://en.wikipedia.org/wiki/RF_power_amplifier" \o "RF power amplifier) and [matching network](https://en.wikipedia.org/wiki/Matching_network" \o "Matching network)
  + [WEP](https://en.wikipedia.org/wiki/Wired_Equivalent_Privacy" \o "Wired Equivalent Privacy) or [WPA/WPA2](https://en.wikipedia.org/wiki/Wi-Fi_Protected_Access" \o "Wi-Fi Protected Access) authentication, or open networks
* 17 [GPIO](https://en.wikipedia.org/wiki/General-purpose_input/output" \o "General-purpose input/output) pins[[7]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-7)
* [Serial Peripheral Interface Bus](https://en.wikipedia.org/wiki/Serial_Peripheral_Interface_Bus" \o "Serial Peripheral Interface Bus) (SPI)
* [I²C](https://en.wikipedia.org/wiki/I%C2%B2C" \o "I²C) (software implementation)[[8]](https://en.wikipedia.org/wiki/ESP8266" \l "cite_note-EspressifBBS_I2C-8)
* [I²S](https://en.wikipedia.org/wiki/I%C2%B2S" \o "I²S) interfaces with DMA (sharing pins with GPIO)
* [UART](https://en.wikipedia.org/wiki/Universal_asynchronous_receiver/transmitter" \o "Universal asynchronous receiver/transmitter) on dedicated pins, plus a transmit-only UART can be enabled on GPIO2
* 10-bit [ADC](https://en.wikipedia.org/wiki/Analog-to-digital_converter" \o "Analog-to-digital converter) ([successive approximation ADC](https://en.wikipedia.org/wiki/Successive_approximation_ADC" \o "Successive approximation ADC))

## Pinout of ESP-01

[](https://en.wikipedia.org/wiki/File:ESP8266_01_PinOut.png)[[edit](https://en.wikipedia.org/w/index.php?title=ESP8266&action=edit&section=2" \o "Edit section: Pinout of ESP-01)]

N.ESP-01 module pinout

The [pinout](https://en.wikipedia.org/wiki/Pinout" \o "Pinout) is as follows for the common ESP-01 module:

1. GND, Ground (0 V)
2. GPIO 2, General-purpose input/output No. 2
3. GPIO 0, General-purpose input/output No. 0
4. RX, Receive data in, also GPIO3
5. VCC, Voltage (+3.3 V; can handle up to 3.6 V)
6. RST, Reset
7. CH\_PD, Chip power-down
8. TX, Transmit data out, also GPIO1

O.ESP 8266

### 5.2 SOFTWARE REQUIREMENTS

The software ecosystem for this system includes tools for programming the microcontroller and simulating or extending the functionality:

**5.2(I) Arduino IDE**

The Arduino IDE (Integrated Development Environment) is a free, open-source software designed for writing, compiling, and uploading code to Arduino boards. It's based on the Processing programming language and provides a user-friendly interface for interacting with Arduino hardware.

Key Features and Concepts:

**Code Editor:**

The IDE includes a text editor where you write your Arduino code (sketches).

**Sketchbook:**

The IDE uses the concept of a sketchbook, a designated folder where your Arduino programs (sketches) are stored.

**Compiler:**

The IDE's compiler translates your C/C++ code into a format that the Arduino microcontroller can understand.

**Uploader:**

The IDE's uploader transmits the compiled code to the Arduino board via a USB connection.

**Libraries:**

The IDE provides access to a vast collection of libraries, which are pre-written code snippets that simplify common tasks.

**Serial Monitor:**

The IDE's serial monitor allows you to communicate with your Arduino board and view data it's sending.

**Board and Port Selection:**

Before uploading code, you need to select the correct Arduino board type and the COM port it's connected to.

**Sketch Structure:**

Arduino sketches typically have two main functions: setup() which runs once at the beginning, and loop() which runs repeatedly.

**Using the IDE:**

**Installation:** Download and install the [Arduino IDE](https://www.arduino.cc/en/software) on your computer.

**Open a Sketch:** Open a new sketch or open an existing one from your sketchbook.

**Write Code:** Write your Arduino code in the code editor.

**Verify:** Use the "Verify" button to check your code for syntax errors.

**Upload:** Use the "Upload" button to compile and upload your code to the Arduino board.

**Serial Monitor:** Use the serial monitor to interact with your Arduino board and view output.

**Benefits of Using the Arduino IDE:**

**Ease of Use:** The IDE is designed to be user-friendly, making it accessible to beginners.

**Cross-Platform Compatibility:** The IDE is available for Windows, macOS, and Linux.

**Open-Source and Free:** The IDE is free to download and use.

**Large Community Support:** The Arduino community offers a wealth of resources and support for users.

P. **Arduino IDE**

**5.2(II) Embedded C and C++:**

Embedded C and C++ are programming languages tailored for embedded systems, which are computer systems embedded within other devices. They offer a balance between low-level control and high-level abstractions, making them suitable for resource-constrained environments with real-time requirements. C++ provides features like object-oriented programming, while C offers simplicity and direct hardware access.

Key Theoretical Concepts:

**Embedded Systems:**

Embedded systems are computer systems embedded within other devices (e.g., cars, appliances, medical devices) to perform specific functions

.

**C and C++ in Embedded Systems:**

Both languages are used in embedded development due to their ability to provide low-level control and efficiency. C++ offers features like object-oriented programming, while C provides a more straightforward approach.

**Object-Oriented Programming (OOP):**

C++ supports OOP, allowing developers to organize code into classes and objects, promoting modularity and reusability.

**Memory Management:**

In embedded systems, efficient memory management is crucial. C and C++ provide different approaches to memory allocation and deallocation.

**Interrupts and Real-Time Systems:**

Embedded systems often require handling interrupts to respond to external events in real-time. C and C++ provide mechanisms for managing interrupts and ensuring real-time responsiveness.

**Hardware Abstraction:**

C and C++ allow developers to abstract away hardware details and interact with hardware components using programming constructs.

**Resource Constraints:**

Embedded systems often operate under resource constraints (memory, processing power). C and C++ offer ways to optimize code for size and speed.

**Low-Level Programming:**

Embedded systems often require direct interaction with hardware, such as accessing memory registers or controlling peripherals. C and C++ provide mechanisms for low-level programming.

**Embedded C++ (EC++):**

EC++ is a subset of C++ designed for embedded systems, focusing on minimizing code size and maximizing execution efficiency while preserving useful object-oriented features.

**Embedded C:**

Embedded C is a set of language extensions for the C programming language, addressing common issues in embedded systems.

C++ Advantages:

**Object-Oriented Paradigm:** C++ supports OOP, making it easier to design and maintain complex embedded systems.

**Abstraction:** C++ allows developers to abstract away hardware details, simplifying the development process.

**Portability:** C++ code can be more portable across different hardware platforms.

**Generic Programming:** C++ supports generic programming, enabling developers to create reusable code for different data types.

**Standard Template Library (STL):** C++ provides a powerful STL for efficient data structures and algorithms.

C Advantages:

**Simplicity:**

C is a simpler language compared to C++, making it easier to learn and use.

**Direct Hardware Access:**

C allows developers to access hardware directly, which can be crucial in embedded systems.

**Resource Efficiency:**

C can be more efficient in terms of code size and memory usage.

**Long History and Support:**

C has a long history in embedded systems, with a vast ecosystem of resources and tools.

Choosing C or C++:

The choice between C and C++ depends on the specific project requirements and constraints. C++ is generally preferred for complex projects that require object-oriented programming and code reuse. C is often preferred for resource-constrained environments where simplicity and direct hardware access are paramount.

### ****\*Libraries:****

### ✅ ****Essential Arduino Libraries****

**1.LiquidCrystal.h**

* Used for standard 16x2 LCD display (parallel interface).
* Required if you're not using an I2C interface.
* Installed by default in the Arduino IDE.

**2.LiquidCrystal\_I2C.h**

* Used for LCDs with an I2C module (2-wire interface).
* Makes wiring easier and reduces pin usage on Arduino.
* Must be installed via **Library Manager** or ZIP file:
* From IDE: Sketch → Include Library → Manage Libraries → Search "LiquidCrystal I2C".

**3.Wire.h**

* Required for I2C communication between Arduino and LCD module.
* Typically used internally by LiquidCrystal\_I2C.

**4.EEPROM.h (Optional)**

* Used if you want to store previous detection counts or thresholds permanently in memory.
* Example: Save how many times alcohol was detected.

### ✅ ****Optional/Extended Functionality Libraries****

If you plan to integrate advanced features like alerts or IoT, you may use:

**1.SoftwareSerial.h**

* Allows multiple serial communication lines (used for modules like GSM or Bluetooth).

**2.ESP8266WiFi.h or WiFi.h**

* If you're using an ESP8266/ESP32 module to connect to the internet.


**3.Adafruit\_Sensor.h (for advanced sensors)**


* Not needed for MQ-3, but good for future extension with other sensors.


**4.Adafruit\_LiquidCrystal.h (Only if using Adafruit’s LCDs)**

* Similar to LiquidCrystal\_I2C.h but specific to Adafruit hardware.

**6.ARCHITECTURE DIAGRAMS**

**6.1 CIRCUIT DIAGRAM**

**6.2 SCHEMATIC DIAGRAM**

**6.3 USE CASE DIAGRAM**

**6.4 EXPLAINATION**

In this alcohol detection and vehicle control system, multiple components are interfaced with the Arduino UNO to detect alcohol presence, alert the user, and control vehicle operation based on sensor readings. Let’s break down the connections in detail.

The core of the project is the **MQ-3 alcohol sensor**, which detects the presence of alcohol vapors in the driver's breath. Its **VCC** pin is connected to the **5V output** of the Arduino to power the sensor, while its **GND** is connected to the **Arduino's ground (GND)** to complete the circuit. The analog signal output from the sensor is connected to **A0** on the Arduino, allowing the microcontroller to read the alcohol level as an analog voltage.

A **16x2 LCD display with an I2C interface** is used to show real-time system messages and alcohol levels. The I2C module simplifies wiring using only two pins: **SDA** and **SCL**, which are connected to the **A4** and **A5** pins of the Arduino respectively. The display’s **VCC** and **GND** pins are connected to **5V** and **GND** to power the module.

To keep track of real-world time (especially for logging or time-stamping alcohol detections), a **DS3231 RTC (Real-Time Clock)** module is connected using the same I2C lines as the LCD. Its **SDA and SCL** lines also go to **A4 and A5**, demonstrating the shared I2C bus feature. Power and ground are similarly connected to **5V and GND**.

A **buzzer** and an **LED** provide auditory and visual alerts. The **buzzer’s positive terminal** is connected to **digital pin D8** on the Arduino and the **negative terminal** to **GND**. When alcohol is detected, the Arduino sends a signal to D8, activating the buzzer. Similarly, an **LED** is used, with its **anode connected through a 220-ohm resistor to D7**, and its **cathode to GND**. This LED lights up when alcohol is detected, acting as a warning indicator.

The system includes a **Wi-Fi module (ESP8266)** to transmit data to a remote server or web application. The module is powered by **3.3V**, as it is not compatible with 5V. Its **TX pin** connects to **Arduino D2**, and its **RX pin** to **D3**, but a **voltage divider circuit** is used to step down the 5V signal from Arduino to 3.3V for the ESP’s RX. The **CH\_PD (or EN)** pin is also connected to **3.3V** to enable the module.

To control the vehicle’s operation, a **relay module** is integrated. The **relay IN pin** is connected to **D6** on the Arduino, allowing it to be triggered based on alcohol detection. The relay acts as a switch that can either allow or block current from a **9V battery** to a **DC motor**. The **COM pin** of the relay connects to one terminal of the motor, and the **NO (Normally Open)** pin connects to the **positive terminal** of the 9V battery. The **other motor terminal** is directly connected to the **negative of the battery**, forming a complete circuit. When alcohol is detected, the relay is **not triggered**, thus **cutting power to the motor** and effectively stopping the vehicle.

This setup ensures a layered safety mechanism: the system not only **detects alcohol levels** but also provides **clear alerts**, **logs events with timestamps**, and **controls vehicle operation**—all while maintaining **wireless data communication** through the ESP8266 module. The use of an I2C LCD and RTC simplifies connections and enhances system scalability.

The alcohol detection and vehicle control system is designed to ensure road safety by preventing intoxicated individuals from operating a vehicle. The primary user of the system is the **driver**, who is required to blow into an alcohol sensor before attempting to start the vehicle. This initial action activates the **Blow Into Sensor** function, which in turn triggers the **Alcohol Sensor System** to detect and evaluate the presence of alcohol in the driver’s breath. If alcohol is detected above a predefined threshold, the system proceeds with the **Detect Alcohol Level** function and evaluates whether it is safe to start the vehicle. In case of a safe reading, the **Start Vehicle** function is activated, enabling engine ignition. However, if the alcohol content is beyond the permissible limit, the system prevents the vehicle from starting or disables it if already running. Simultaneously, a **Send Alert Notification** function is triggered through the **Notification System**, which sends a real-time alert (such as SMS or email) to a registered **guardian** or emergency contact.

The system further enhances safety with the **Trigger Alarm** function, which activates a buzzer to audibly alert the driver and others nearby about the safety breach. This action is a part of the **Vehicle Control System**, which works closely with the alcohol sensor. Additionally, the **Disable Engine** function is employed either to prevent the car from starting initially or to gradually slow down and stop the vehicle if intoxication is detected while driving. To maintain accountability and assist in future monitoring, the system executes the **Update Stats** function, which logs the alcohol reading, time, date, and number of violations to a central database or cloud-based platform. This data is accessible by the **guardian**, who can use the **See Stats** function to analyze patterns and respond appropriately.

Through these interconnected functions, the system ensures a multi-layered approach to vehicle safety, integrating real-time alcohol detection, vehicle control measures, alert notifications, and statistical monitoring. This not only helps in preventing accidents caused by drunk driving but also keeps guardians informed, making it a robust safety mechanism. The overall system design represents an integration of hardware components like sensors, buzzers, and relays with intelligent software handling decision-making, notifications, and data tracking. Thus, this project offers an effective solution to tackle the serious issue of drunk driving through automation and accountability.

**6.5 SUMMARY TABLE**

| **Component** | **Pin** | **Connected To** | **Purpose** |
| --- | --- | --- | --- |
| **MQ-3 Alcohol Sensor** | VCC | 5V (Arduino) | Power supply for sensor |
|  | GND | GND (Arduino) | Common ground |
|  | A0 | A0 (Arduino) | Analog output signal to Arduino |
| **16x2 I2C LCD** | VCC | 5V (Arduino) | Power supply for LCD |
|  | GND | GND (Arduino) | Common ground |
|  | SDA | A4 (Arduino) | I2C Data line |
|  | SCL | A5 (Arduino) | I2C Clock line |
| **LED** | Anode (+) | 220Ω Resistor → D7 | Visual alert when alcohol is detected |
|  | Cathode (–) | GND (Arduino) | Common ground |
| **Buzzer** | + (Positive) | D8 (Arduino) | Audible alert when alcohol is detected |
|  | – (Negative) | GND (Arduino) | Common ground |
| **ESP8266 Wi-Fi Module** | TX | D2 (Arduino) | Transmits data from ESP to Arduino |
|  | RX | D3 (Arduino via voltage divider) | Receives data from Arduino |
|  | VCC | 3.3V (Arduino) | Power supply (ESP is 3.3V only) |
|  | GND | GND (Arduino) | Common ground |
|  | CH\_PD / EN | 3.3V (Arduino) | Enable pin to activate ESP8266 |
| **Relay Module** | IN | D6 (Arduino) | Trigger relay from Arduino |
|  | VCC | 5V (Arduino) | Power supply for relay coil |
|  | GND | GND (Arduino) | Common ground |
|  | COM | One motor terminal | Relay's common switch line |
|  | NO (Normally Open) | 9V Battery (+) | Supplies power when relay is active |
| **DC Motor** | Terminal 1 | COM (Relay) | Power through relay control |
|  | Terminal 2 | 9V Battery (–) | Completes power loop |

**7.MODULES**

## HARDWARE MODULES

### 1. ****Arduino Uno:****

The **Arduino Uno** is the central microcontroller unit that governs all the operations in the system. It receives analog signals from the alcohol sensor (MQ-3), processes this data, and decides whether the output devices like the buzzer, LED, relay module, and motor should be activated or not. It also controls the messages displayed on the LCD screen and communicates with external modules like Wi-Fi if internet connectivity is enabled. The Arduino acts like the "brain" of the system and executes all the decision-making logic through a program written in the Arduino IDE.

### 2. ****MQ-3 Alcohol Sensor****

The **MQ-3 sensor** is responsible for detecting the presence and concentration of alcohol vapors in the air. It contains a heating element and sensing layer made of tin dioxide (SnO₂), which reacts with alcohol vapors. As alcohol concentration increases, the sensor's resistance decreases, altering the output voltage. The analog signal from the MQ-3 is read by the Arduino. If the alcohol level is above a certain threshold, the Arduino triggers alerts and disables the vehicle control system. This sensor is highly sensitive to ethanol and is commonly used for breath analyzers.

### 3. ****Buzzer****

The **buzzer** acts as an audible alert system. When the MQ-3 detects alcohol levels beyond the permissible threshold, the Arduino activates the buzzer. This acts as a warning to the driver and surrounding passengers, making them aware that the system has detected a possible alcohol consumption. It adds an extra layer of safety by drawing immediate attention to the situation.

### 4. ****Relay Module****

The **relay module** works as a digital switch, controlled by the Arduino. It is used to cut off the power supply to the motor (which simulates the engine). When alcohol is detected, the Arduino sends a signal to the relay, which then opens the circuit and stops the engine. This module ensures that the vehicle cannot be started or driven under the influence of alcohol. It plays a vital role in real-world vehicle immobilization applications.

### 5. ****DC Motor****

The **DC motor** is used in the project to simulate the operation of a vehicle’s engine. It is connected to the relay module and powered through the Arduino’s control system. When alcohol is detected, the motor is turned off to simulate stopping the engine, representing how the vehicle control system would respond in a real-world scenario.

### 6. ****LED****

The **LED** is a simple yet effective output component used to give visual indications of the system status. When alcohol is detected, the Arduino turns the LED ON, providing a quick and easily noticeable alert in addition to the buzzer. This dual alert system (audio + visual) enhances safety and awareness.

### 7. ****16x2 LCD Display (with I2C Interface)****

The **16x2 LCD display** is used to provide textual feedback to the driver. Messages such as “Blow into the sensor,” “Alcohol Detected,” or “Vehicle Starting…” are shown to guide the driver through the system’s processes. The I2C interface allows for easier wiring using just two Arduino pins (SDA and SCL) for communication, reducing complexity and saving GPIO pins.

### 8. ****Power Supply Module****

A **power supply module** provides the necessary electrical energy to run the Arduino and other connected modules. Depending on the project setup, it could be powered using USB, a battery pack, or an adapter. Stability of the power supply is important to ensure accurate sensor readings and consistent system behavior.

### 9. ****Wi-Fi Module / NodeMCU (Optional)****

In the enhanced version of the project, a **Wi-Fi module** such as the **NodeMCU** or **ESP8266** can be used to connect the system to the internet. It enables features like sending real-time notifications via email or SMS to a guardian or hospital if the alcohol level is high. It also allows remote monitoring and control through a web-based dashboard.

## 7.2 SOFTWARE &CLOUD MODULES

### 10. ****Arduino IDE****

The **Arduino IDE** is the software used to write and upload the program (sketch) to the Arduino Uno. The code includes logic for reading the alcohol sensor values, comparing them with a predefined threshold, activating or deactivating the buzzer and relay, and displaying messages on the LCD. It also contains the timing and control logic for periodic sensor checks and user interaction instructions.

### 11. ****Web Application (Frontend Interface)****

A **web-based interface** is used to visualize the system’s historical data, such as the number of alcohol detections, timestamps, and user behavior patterns. The interface is user-friendly and can display interactive graphs, alerts, and notifications. Guardians or authorities can access this dashboard to monitor the driver's status in real time.

### 12. ****Cloud Database (e.g., Firebase or ThingSpeak)****

A **cloud database** is used to store the alcohol sensor readings along with timestamps and event logs. This data can be retrieved and analyzed to detect patterns or repeated violations. When integrated with the frontend, it enhances the effectiveness of the monitoring system, allowing for real-time updates and future analytics.

**8.IMPLEMENTATION**

The implementation phase of the Alcohol Detection and Vehicle Control System is where theoretical planning transitions into practical realization. This stage involves setting up the hardware components, writing and uploading the embedded code, assembling the circuit, and testing the system in real-time conditions to validate its reliability and responsiveness. The goal is to create a responsive, accurate, and efficient embedded system that can monitor a driver's sobriety level and take automated decisions to control the vehicle accordingly.

### 8.1 HARDWARE ASSEMBLY

The hardware implementation begins with laying out the components on a breadboard for testing. The MQ-3 gas sensor is the core component responsible for detecting ethanol vapor from the driver's breath. It is connected to the analog input pin A1 of the Arduino Uno. This sensor is sensitive to alcohol concentration and generates an analog voltage that increases proportionally with the presence of alcohol in the surrounding air. For proper functioning, the sensor needs a short warm-up period, usually 20–30 seconds.

The Arduino Uno acts as the processing unit of the system. It takes input from the MQ-3 sensor and performs decision-making based on the programmed threshold values. The board uses digital output pins to control peripherals such as a relay module, buzzer, and LED. Pin 9 is designated for the relay, pin 7 for the buzzer, and pin 8 for the red LED used to indicate danger.

An LCD module (16x2 display) with an I2C interface is included in the setup to provide visual feedback to the driver. Messages such as “Blow into Sensor,” “Alcohol Detected,” “Drive Safe,” or “Vehicle Stopped” are shown depending on the system status. The I2C protocol simplifies wiring and saves GPIO pins on the Arduino, making it ideal for compact designs.

The relay module is used as a switch to simulate the control of the vehicle’s ignition system. When alcohol is detected above a specified level, the relay is deactivated, cutting off power to the motor or ignition, thereby preventing the vehicle from starting or continuing to operate.

To power the system, either a USB cable connected to a computer or a 9V battery with a barrel jack adapter is used. During permanent installations or prototype demonstrations, a regulated adapter ensures continuous and stable power supply.

### 8.2 SOFTWARE DEVELOPMENT

The software development begins with writing code in the Arduino IDE using Embedded C/C++. The program is structured into two major phases: before the vehicle starts and during the vehicle's operation.

In the first phase, the system prompts the driver to blow air near the MQ-3 sensor. The analog value from the sensor is read and compared against a threshold value. If the value exceeds the threshold, the LCD displays an alert, the buzzer is turned on, and the relay cuts power to the motor, preventing the vehicle from starting. If the alcohol level is below the threshold, the LCD displays a green message, and the relay is activated to allow ignition.

In the second phase, the system enters a continuous monitoring mode. While the vehicle is running, the sensor continues to read the alcohol level at fixed intervals. If it detects alcohol during the trip, it triggers an alert and shuts down the vehicle gradually to ensure safety. The system also includes logic to handle ignored readings or attempts to bypass the sensor. It does this by implementing delays and forcing the driver to blow into the sensor again.

The program uses Serial Monitor to print real-time sensor readings for debugging and calibration purposes. This feature is useful during development and testing to determine the best threshold value for alcohol detection under various environmental conditions.

### 8.3 PROTOTYPE DEPLOYMENT

The final prototype is assembled onto a small car chassis for demonstration purposes. The LCD is mounted in a position where it mimics a dashboard display. The MQ-3 sensor is positioned near the driver's face or steering wheel area to replicate real-life usage. The relay is connected to a small DC motor representing the engine, and the entire circuit is powered by a regulated 9V or 12V battery pack.

The system is enclosed in a protective casing to prevent damage during handling. A switch is provided to turn the system on or off as required. During demonstration, the prototype clearly shows how the system blocks the engine from starting when alcohol is detected and how it continues to monitor the driver after the engine is started.

**8.4 CODE**

**#include <Wire.h>**

**#include <LiquidCrystal\_I2C.h>**

**#include <SoftwareSerial.h>**

**// LCD setup**

**LiquidCrystal\_I2C lcd(0x27, 20, 4);**

**// ESP8266 (ESP-01) setup**

**SoftwareSerial espSerial(2, 3); // RX, TX**

**const int mq3Pin = A0;**

**const int relayPin = 8;**

**const int buzzerPin = 7;**

**const int ledPin = 9;**

**const int alcoholThreshold = 400;**

**// WiFi & ThingSpeak**

**const char\* ssid = "OPPO A12";**

**const char\* password = "12345678";**

**const char\* apiKey = "IQQM8HX9RVHZ21RB";**

**void setup() {**

**pinMode(relayPin, OUTPUT);**

**pinMode(buzzerPin, OUTPUT);**

**pinMode(ledPin, OUTPUT);**

**digitalWrite(relayPin, HIGH); // Motor OFF**

**digitalWrite(buzzerPin, LOW);**

**digitalWrite(ledPin, LOW);**

**lcd.init();**

**lcd.backlight();**

**Serial.begin(9600);**

**espSerial.begin(115200);**

**connectToWiFi();**

**}**

**void connectToWiFi() {**

**espSerial.println("AT+RST");**

**delay(2000);**

**espSerial.println("AT+CWMODE=1");**

**delay(2000);**

**String cmd = "AT+CWJAP=\"" + String(ssid) + "\",\"" + String(password) + "\"";**

**espSerial.println(cmd);**

**delay(5000); // Wait for WiFi connection**

**}**

**void sendToThingSpeak(int value) {**

**String cmd = "AT+CIPSTART=\"TCP\",\"api.thingspeak.com\",80";**

**espSerial.println(cmd);**

**delay(2000);**

**String httpCmd = "GET /update?api\_key=" + String(apiKey) + "&field1=" + String(value) + "\r\n";**

**int length = httpCmd.length() + 4;**

**espSerial.print("AT+CIPSEND=");**

**espSerial.println(length);**

**delay(1000);**

**espSerial.print(httpCmd);**

**delay(1500);**

**espSerial.println("AT+CIPCLOSE");**

**delay(1000);**

**}**

**void phase1() {**

**lcd.clear();**

**lcd.setCursor(2, 0);**

**lcd.print("ALCOHOL DETECTION");**

**lcd.setCursor(6, 1);**

**lcd.print("SYSTEM");**

**delay(3000);**

**lcd.clear();**

**lcd.setCursor(3, 1);**

**lcd.print("Blow into sensor");**

**delay(2000);**

**int sensorValue = analogRead(mq3Pin);**

**sendToThingSpeak(sensorValue); // <=== Send to ThingSpeak**

**if (sensorValue > alcoholThreshold) {**

**digitalWrite(relayPin, HIGH);**

**digitalWrite(buzzerPin, HIGH);**

**digitalWrite(ledPin, HIGH);**

**lcd.clear();**

**lcd.setCursor(1, 1);**

**lcd.print("Alcohol detected");**

**lcd.setCursor(0, 2);**

**lcd.print("Car won't start");**

**delay(5000);**

**digitalWrite(buzzerPin, LOW);**

**digitalWrite(ledPin, LOW);**

**} else {**

**digitalWrite(relayPin, LOW);**

**digitalWrite(buzzerPin, LOW);**

**digitalWrite(ledPin, LOW);**

**lcd.clear();**

**lcd.setCursor(5, 1);**

**lcd.print("Safe to drive");**

**delay(5000);**

**}**

**}**

**void phase2() {**

**while (true) {**

**lcd.clear();**

**lcd.setCursor(3, 1);**

**lcd.print("Blow into sensor");**

**delay(2000);**

**int sensorValue = analogRead(mq3Pin);**

**sendToThingSpeak(sensorValue); // <=== Send to ThingSpeak**

**if (sensorValue > alcoholThreshold) {**

**digitalWrite(buzzerPin, HIGH);**

**digitalWrite(ledPin, HIGH);**

**lcd.clear();**

**lcd.setCursor(1, 1);**

**lcd.print("Alcohol detected");**

**lcd.setCursor(0, 2);**

**lcd.print("Stopping the car");**

**digitalWrite(relayPin, HIGH); // Stop car**

**delay(10000);**

**digitalWrite(buzzerPin, LOW);**

**digitalWrite(ledPin, LOW);**

**} else {**

**digitalWrite(relayPin, LOW);**

**digitalWrite(buzzerPin, LOW);**

**digitalWrite(ledPin, LOW);**

**lcd.clear();**

**lcd.setCursor(5, 1);**

**lcd.print("Safe to drive");**

**delay(15000);**

**}**

**}**

**}**

**void loop() {**


**phase1();**

**delay(10000);**


**phase2();**

**}**


**9.SCREENSHOTS**


****

**9.1 prompt display**


****

**9.2 phase 1 blow into sensor**


****

**9.3 safe to drive prompt**


**9.4 phase 2 blow into sensor**

****


**9.5 alcohol detected (motor slowing down )**

****

**9.6 alcohol detected (motor stop )**



**9.7 alcohol detected 1**



**9.8 alcohol detected 2**

**10.TESTING**

Testing is a critical phase in the development of the Alcohol Detection and Vehicle Control System. This stage ensures that all the functionalities of the system operate as intended and respond appropriately to real-world scenarios. Various testing strategies were employed to evaluate the system’s performance, accuracy, stability, and reliability.

### 10.1 UNIT TESTING

Unit testing focuses on validating individual components or modules of the system in isolation. Each part of the project—such as the MQ-3 alcohol sensor, LCD display, buzzer, and relay—was tested separately before integrating them into the final prototype.

* **MQ-3 Sensor** was tested by measuring analog outputs with varying alcohol exposure.
* **LCD Display** was tested with sample messages to ensure accurate character rendering.
* **Relay Module** was triggered using simple high/low commands to verify its switching mechanism.
* **Buzzer and LED** were tested by applying digital outputs to check audio and visual alerts.

### 10.2 INTEGRATION TESTING

After confirming individual component performance, integration testing was performed. This involved connecting all modules together and observing how they functioned collectively:

* The sensor output was fed to the Arduino to determine the decision logic.
* Outputs from Arduino were verified to activate/deactivate the relay, buzzer, and LED.
* The LCD was cross-checked to display the correct message corresponding to sensor readings.

### 10.3 SYSTEM TESTING

In system testing, the fully integrated prototype was evaluated as a whole under realistic conditions. The test environment simulated a vehicle dashboard with proper spacing for components.

Scenarios tested included:

* Driver blowing into the sensor with no alcohol — system allowed engine start.
* Driver blowing with alcohol presence — system blocked engine, activated alarm.
* Monitoring during travel — system detected alcohol mid-journey and shut down the motor.

### 10.4 VALIDATION AND THRESHOLD TUNING

The sensor’s analog output was observed under different alcohol concentrations. Using Serial Monitor, threshold values were adjusted dynamically to fine-tune the detection accuracy. The optimal threshold (e.g., 400–500) was selected where the system balanced sensitivity and false positives.

Alcohol exposure was simulated using:

* Hand sanitizers
* Spirit-based cologne
* Mild ethanol sprays

### 10.5 PERFORMANCE EVALUTION

* **Response Time:** The system responded within 1-2 seconds of detecting alcohol.
* **Accuracy:** It consistently detected presence/absence of alcohol under repeated trials.
* **Stability:** The system functioned without crashing or freezing under extended usage.

### 10.6 USER ACCEPTENCE TEST(UAT)

To test usability and clarity, the system was presented to peers and evaluators. Feedback was collected regarding:

* Message clarity on the LCD screen
* Sound volume of buzzer
* Effectiveness of LED indicator

Changes were made based on feedback, such as increasing LCD delay time and optimizing alert durations.

### 10.7 CONCLUSION OF TESTING PHASE

All critical functionalities of the Alcohol Detection and Vehicle Control System passed their respective tests. From sensor calibration to full system response, the prototype demonstrated reliability, robustness, and clear user feedback mechanisms. The successful testing phase confirms that the system is ready for demonstration, documentation, and potential future scaling.

**11.CONCLUSION**

The Alcohol Detection and Vehicle Control System is a practical solution designed to prevent drunk driving incidents through real-time alcohol monitoring. This project was inspired by the growing need to address traffic accidents caused by impaired driving, and it combines essential hardware and software elements to detect alcohol concentration and control vehicle ignition accordingly. The system utilizes the MQ-3 gas sensor, which detects ethanol vapors from a driver's breath, an Arduino Uno microcontroller to process sensor input, and peripheral components like a buzzer, relay, and LCD display to communicate system status and enforce vehicle control.

Throughout the design and development process, an emphasis was placed on creating a simple yet effective embedded system capable of handling real-time sensor input and executing rapid decision-making logic. The LCD provides clear driver feedback, the buzzer offers immediate alerts in the case of alcohol detection, and the relay acts as a switch to control motor operation, simulating engine shutdown. Together, these components offer a holistic safety mechanism designed to prevent vehicles from operating under unsafe conditions.

Implementation of this project involved setting up both the electronic circuitry and the software logic that governs the system’s behavior. During pre-ignition checks, the system ensures that the driver is sober before allowing the engine to start. While driving, continuous monitoring ensures that any alcohol consumption mid-journey results in a system-triggered engine cutoff. This continuous monitoring mechanism is a key safety feature, enhancing the system's relevance and practicality in real-world applications.

Extensive testing validated the system's accuracy, responsiveness, and reliability. The analog output of the MQ-3 sensor was tested under various conditions to fine-tune its sensitivity, while system performance was analyzed for delay, false positives, and component behavior under stress. As a result, the system was calibrated to react quickly and minimize operational error, ensuring a reliable safety net for drivers and passengers.

From a technical perspective, the project reinforces key embedded systems concepts including sensor integration, real-time decision-making, actuator control, and user feedback mechanisms. The hardware-software co-design allowed for a modular and scalable system architecture, which opens the possibility of future expansions such as integration with IoT modules (ESP8266/ESP32), GPS tracking for emergency response, and mobile app-based alerts.

Socially, the project addresses a pressing issue in road safety by promoting responsible driving behavior. If implemented on a larger scale, especially in commercial fleets or public transportation vehicles, the technology could reduce DUI incidents, protect lives, and support legal enforcement of safety regulations.

In conclusion, the Alcohol Detection and Vehicle Control System is an innovative and efficient project that successfully integrates sensor technology, microcontroller programming, and user-centric design to deliver a working prototype aimed at saving lives. Its success in both functionality and usability validates the feasibility of such safety systems being adopted into future intelligent vehicle ecosystems.

**12.REFERENCES**

**PUBLISHED RESEARCH PAPERS :**

* H. B. Noris et al., "Alcohol Detection Using Breath Analyzers and Microcontrollers: A Review," International Journal of Advanced Research in Electronics and Communication Engineering (IJARECE), vol. 4, no. 3, pp. 755-760, March 2015.
* R. Sharma and A. Yadav, "Smart Alcohol Detection and Ignition Locking System for Vehicles Using IoT," International Journal of Engineering Research & Technology (IJERT), vol. 6, no. 8, pp. 442-445, Aug. 2017.
* P. R. Deshmukh et al., "Drunken Driving Detection and Vehicle Control System Using GSM and GPS," International Journal of Scientific Research in Science, Engineering and Technology, vol. 8, no. 2, pp. 123-128, Feb. 2022.

**TEXTBOOKS :**

* M. A. Mazidi, R. D. McKinlay, and D. Causey, Programming and Customizing the AVR Microcontroller, McGraw-Hill, 2007.
* Muhammad Ali Mazidi and Janice Gillispie Mazidi, The 8051 Microcontroller and Embedded Systems: Using Assembly and C, Pearson Education, 2012.
* Raj Kamal, Embedded Systems: Architecture, Programming and Design, McGraw-Hill Education, 3rd Edition, 2017.

**WEBLINKS:**

* MQ-3 Alcohol Sensor Datasheet – <https://www.sparkfun.com/datasheets/Sensors/MQ-3.pdf>
* Arduino Uno Technical Specifications – <https://store.arduino.cc/products/arduino-uno-rev3>
* LiquidCrystal\_I2C Library Documentation – <https://github.com/johnrickman/LiquidCrystal_I2C>
* Relay Module with Arduino Tutorial – <https://randomnerdtutorials.com/guide-for-relay-module-with-arduino/>
* Arduino IDE Software – <https://www.arduino.cc/en/software>
* WHO Road Safety Facts – <https://www.who.int/news-room/fact-sheets/detail/road-traffic-injuries>
* Adafruit LCD Library and Tutorials – <https://learn.adafruit.com/character-lcds>
* Tinkercad Arduino Simulator – <https://www.tinkercad.com/>
* Introduction to Embedded Systems – <https://www.geeksforgeeks.org/introduction-to-embedded-systems/>
* DADSS Program - Driver Alcohol Detection System for Safety – <https://www.dadss.org/>

**Abstract**

Driving under the influence (DUI) of alcohol remains a critical public safety issue worldwide, contributing to a significant percentage of road traffic accidents, injuries, and fatalities. Despite numerous awareness campaigns and strict legal penalties, instances of drunk driving persist due to the lack of real-time enforcement mechanisms. This project titled "Alcohol Detection and Vehicle Control System Using Arduino" aims to provide a technological solution to this ongoing challenge by designing a smart, real-time, embedded system that can detect alcohol consumption by the driver and immediately prevent vehicle operation if intoxication is detected.

The project utilizes an Arduino Uno microcontroller as the central processing unit, interfaced with an MQ-3 alcohol sensor to detect ethanol vapor in the driver's breath. This sensor provides an analog output proportional to the concentration of alcohol, which is then processed by the Arduino. Upon exceeding a predefined threshold level, the system performs a series of safety interventions: a relay module is triggered to disable the vehicle's ignition (represented in this model by a DC motor), a buzzer is activated to provide an audible warning, and a 16x2 I2C LCD displays visual alerts indicating the detection of alcohol and denial of vehicle access. If no alcohol is detected, the vehicle is allowed to start normally, and the system displays a "Safe to Drive" message.

To ensure a compact and efficient design, the entire system is powered using a rechargeable 18650 lithium-ion battery. Power distribution is carefully managed to provide sufficient and stable voltage to all modules. The architecture incorporates essential safety features, including a relay to electrically isolate the microcontroller from the high-current motor circuit, thereby protecting the electronics from voltage spikes. The use of I2C communication for the LCD ensures minimal pin usage and allows for future expansion of the system.

This system's primary goal is to act as a preventive mechanism rather than a reactive one, halting the possibility of drunk driving before the vehicle even starts. Its modular design allows for a wide range of enhancements such as integration with GSM modules for emergency alerts, GPS for real-time location tracking, data logging for historical analysis, and IoT-based cloud connectivity for remote monitoring by authorities or guardians. With the addition of biometric verification methods like fingerprint recognition, the system can be adapted for fleet management and personal vehicle safety applications.

The Alcohol Detection and Vehicle Control System serves as a cost-effective, scalable, and reliable tool for combating the dangers of drunk driving. It demonstrates the power of embedded systems in addressing social issues and enhancing human safety through automation. By leveraging simple yet effective hardware components and intelligent programming, the project offers an innovative and deployable solution that can be implemented in both commercial and personal vehicles.

In conclusion, this system represents a step forward in integrating technology into road safety enforcement. It not only reinforces the legal and ethical standards against drunk driving but also introduces a tangible, user-friendly intervention capable of saving countless lives by ensuring that no intoxicated individual is able to operate a vehicle.